

**CONSTRUCTION PRODUCTS REGULATION**

**DECLARATION OF PERFORMANCE**

**No: 565/1-CPR/ 2014**

Substrate: Mortar M1 and Anodised aluminium

Primer: No primer

|  |  |
| --- | --- |
| 1. Identification Code | **Everbuild 565 Clean Room Silicone****Codes: 565WE** |
| 2. Type, Batch and/or Serial Number | **- For batch number - see packaging** |
| 3. Intended use | **Sealant for non-structural use in joints in buildings and pedestrian walkways Part 1: Sealants for Façade elements** |
| 4. Manufacturer | **Everbuild Building Products ltd, Site 41, Cross Green Industrial Estate, Knowsthorpe Way, Leeds, LS9 0SW** |
| 5. Authorised Representative | **Not Applicable** |
| 6. Assessment and Verification of Constancy of Performance | **System 3** |
| 7. Notified Body and Tasks | **SKZ Notified Body No. 1213** |
| 8. European Technical Assessment | **Not Applicable** |
| 9. Declared Performance **TO EN15651-1 (2012)**  |
| Type | **F EXT-INT-CC** |
| Classification | **F25LM** |
| Reaction to Fire | **Class E** |
| Loss of Volume ISO10563 | **≤10%** |
| Resistance to flow ISO7390 | **≤3 mm** |
| Adhesion/cohesion properties at maintained extension after water immersion (23°C) ISO 10590 | **NF** |
| Adhesion/cohesion properties (-30°C) | **≤0.9 MPa** |
| Durability ISO 8340, ISO 9047 and ISO 10590 | **Pass** |

Substrate: Anodised aluminium

Primer: No Primer

|  |  |
| --- | --- |
| 1. Identification Code | **Everbuild 565 Clean Room Silicone****Codes: 565WE** |
| 2. Type, Batch and/or Serial Number | **- For batch number - see packaging** |
| 3. Intended use | **Sealant for non-structural use in joints in buildings and pedestrian walkways Part 3: Sealants for Sanitary elements** |
| 4. Manufacturer | **Everbuild Building Products ltd, Site 41, Cross Green Industrial Estate, Knowsthorpe Way, Leeds, LS9 0SW** |
| 5. Authorised Representative | **Not Applicable** |
| 6. Assessment and Verification of Constancy of Performance | **System 3** |
| 7. Notified Body and Tasks | **SKZ Notified Body No. 1213** |
| 8. European Technical Assessment | **Not Applicable** |
| 9. Declared Performance **TO EN15651-3 (2012)**  |
| Type | **S**  |
| Classification | **XS1** |
| Reaction to Fire | **Class E** |
| Loss of Volume ISO10563 | **≤20%** |
| Resistance to flow ISO7390 | **≤3 mm** |
| Adhesion/cohesion properties at maintained extension after water immersion (23°C) ISO 10590 | **NF** |
| Action of the microorganisms : Intensity of growth ISO 846, method B | **2** |
| Durability ISO 846, method B, ISO 8340, ISO 9047 and ISO 10590 | **Pass** |

The performance of the product identified in points 1 and 2 is in conformity with the declared performance in point 9 . The declaration of performance is issued under the sole responsibility of the manufacturer identified in point 4.

Signed: I. G. Southerington – Head of Technical P.R. Thomas – Technical Manager



Dated: Leeds, 10/6/14